Jump to main content

# 2.1.4.32 DRV_MCMETROLOGY_START_MODE Enum

## C

    typedefenum
    {
        /* Operation completed with success. */
        DRV_MCMETROLOGY_START_SOFT,

        /* Invalid handle or operation failed. */
        DRV_MCMETROLOGY_START_HARD

    } DRV_MCMETROLOGY_START_MODE;

## Summary

Describes how is the start-up process.

## Description

HARD mode implies a full reload of Core 1 firmware. SOFT mode does not have any effect on Core 1 firmware.

Rev: E