Jump to main content

# 1.1.4.43 DRV_METROLOGY_GAIN_TYPE Enum

## C

    typedef enum
    {
        GAIN_1        = 0,
        GAIN_2        = 1,
        GAIN_4        = 2,
        GAIN_8        = 3,
        GAIN_16       = 4,
        GAIN_32       = 5,
        GAIN_NUM_TYPE
    } DRV_METROLOGY_GAIN_TYPE;

## Summary

Gain selected for use in the ADC front-end.

## Remarks

Gain is fixed to 1 on voltage channels.

Gain 16x and 32x are only valid on MCP AFEs, not in ATSENSE.

Rev: E