Jump to main content

# 1.1.4.56 DRV_METROLOGY_CAPTURE_CHN_MASK Enum

## C

    typedef enum {
        CAPTURE_CHN_IA    = 0,
        CAPTURE_CHN_VA    = 1,
        CAPTURE_CHN_IB    = 2,
        CAPTURE_CHN_VB    = 3,
        CAPTURE_CHN_IC    = 4,
        CAPTURE_CHN_VC    = 5,
        CAPTURE_CHN_IN    = 6,
        CAPTURE_CHN_VD    = 7
    } DRV_METROLOGY_CAPTURE_CHN_MASK;

## Summary

Channel identifier used in the waveform capture process.

## Description

Identify the channel to be captured. Up to 7 channels of data may be captured at the same time.

Rev: E