Jump to main content

# 1.1.4.37 DRV_METROLOGY_CaptureCheckIsWrap Function

## C

    bool DRV_METROLOGY_CaptureCheckIsWrap(void);

## Summary

Capture buffer overflown and wrapped.

## Description

Check if buffer used to capture samples has overflown and wrapped at least once.

## Parameters

None.

## Returns

True if the capture buffer has wrapped at least once.

## Example

            if (DRV_METROLOGY_CaptureCheckIsWrap() == true)
            {
                SYS_CMD_MESSAGE("Waveform capture buffer is wrapped\r\n");
            }

## Remarks

None.

Rev: E