Jump to main content

# 3.1.4.18 ICM_DisableInterrupt Function

## C

    void ICM_DisableInterrupt (ICM_INTERRUPT_SOURCE source, ICM_REGION_ID regionId);

## Summary

Clears the interrupt source of a memory region of the ICM peripheral.

## Description

Disables the interrupt source of the memory region with regionId identifier.

## Precondition

None.

## Parameters

Parameters | Description
--- | ---
source | Source of the interrupt to disable
regionId | Identifies the memory region to disable interrupt

## Returns

None.

## Example

    ICM_DisableInterrupt(ICM_INTERRUPT_RDM, ICM_REGION_0);
    ICM_DisableInterrupt(ICM_INTERRUPT_RDM, ICM_REGION_1);

## Remarks

None.

Rev: E