Jump to main content

# 1.1.4.45 DRV_METROLOGY_DOMINANT_V_SEL Enum

## C

    typedef enum
    {
        DOMINANT_V_DYNAMIC = 0,
        DOMINANT_V_PHASE_A = 1,
        DOMINANT_V_PHASE_B = 2,
        DOMINANT_V_PHASE_C = 3,
        DOMINANT_V_NUM
    } DRV_METROLOGY_DOMINANT_V_SEL;

## Summary

Dominant Voltage Selection (SYNCH field in FEATURE_CTRL register).

## Description

These are the allowed values for SYNCH field in FEATURE_CTRL register. It is used for Neutral Current phase calibration, to select which is the voltage channel used as reference.

Rev: E