Jump to main content

# 3.3.4.31 EMAFE_ADCI1Enable Function

## C

    void EMAFE_ADCI1Enable(uint8_t gain);

## Summary

Enable ADC I1.

## Description

Enable ADC I1.

## Precondition

None.

## Parameters

Parameters | Description
--- | ---
gain | Channel I1 Gain Configuration

## Returns

None.

## Example

    EMAFE_ADCI1Enable(EMAFE_ADC_ADCI1_CTRL_GAINX1);

## Remarks

Gain Value | Description
--- | ---
EMAFE_ADC_ADCI1_CTRL_GAINX1 | Input stage of the ADC has a gain of 1
EMAFE_ADC_ADCI1_CTRL_GAINX2 | Input stage of the ADC has a gain of 2
EMAFE_ADC_ADCI1_CTRL_GAINX4 | Input stage of the ADC has a gain of 4
EMAFE_ADC_ADCI1_CTRL_GAINX8 | Input stage of the ADC has a gain of 8

Rev: E