Jump to main content

# 1.1.4.40 DRV_METROLOGY_START_MODE Enum

## C

    typedef enum
    {
        /* Initialize Driver without resetting coprocessor */
        DRV_METROLOGY_START_SOFT,

        /* Initialize Driver and reset coprocessor */
        DRV_METROLOGY_START_HARD

    } DRV_METROLOGY_START_MODE;

## Summary

Describes how is the start-up process regarding coprocessor reset.

## Description

HARD mode implies a full reload of Core 1 firmware. SOFT mode does not have any effect on Core 1 firmware.

Rev: E