Jump to main content

# Status Registers

The status registers can be read by means of the DSR command. Examples:

    ; Read the first metrology status register
    DSR[0]
    00 VERSION
    30400

    ; Read all the metrology status registers
    DSR
    00 VERSION         01 STATUS          02 STATE_FLAG      03 CAPTURE_STATUS
    30400              8                  7000020            FF
    04 INTERVAL_NUM    05 N               06 PH_OFFSET       07 FREQ
    7AC0015            FB2                FF0A3D71           37C62
    08 FREQ_VA         09 FREQ_VB         10 FREQ_VC         11 RESERVED_S11
    3B061              323F0              321F9              0
    12 TEMPERATURE     13 V_A_MAX         14 V_B_MAX         15 V_C_MAX
    14F7               30850              2F0DC              2FD0A
    16 RESERVED_S16    17 I_A_MAX         18 I_B_MAX         19 I_C_MAX
    0                  1D232              23AED              1D7A9
    20 I_Nm_MAX        21 I_Ni_MAX        22 FEATURES        23 N_CYCLE
    105C74             2EAE               807F6E00           4D400
    24 RESERVED_S24    25 RESERVED_S25    26 PULSE0_COUNTER  27 PULSE1_COUNTER
    0                  0                  0                  0
    28 PULSE2_COUNTER  29 RESERVED_S29    30 ZC_N_VA         31 ZC_N_VB
    0                  0                  599380             5ACE00
    32 ZC_N_VC         33 RESERVED_S33    34 ATCAL_41_44     35 ATCAL_45_48
    646400             0                  B401CB03           2602D003

Rev: E