Jump to main content

# 2.1.4.35 DRV_MCMETROLOGY_GAIN_TYPE Enum

## C

    typedefenum
    {
        GAIN_1        = 0,
        GAIN_2        = 1,
        GAIN_4        = 2,
        GAIN_8        = 3,
        GAIN_16       = 4,
        GAIN_32       = 5,
        GAIN_NUM_TYPE
    } DRV_MCMETROLOGY_GAIN_TYPE;

## Summary

Gain selected for use in the ADC front-end.

## Description

On Current measurement channels gain for voltage is fixed to 1.

Rev: E