Jump to main content

# 1.1.4.53 DRV_METROLOGY_MEASURE_TYPE Enum

## C

    typedef enum {
        MEASURE_UA_RMS = 0,
        MEASURE_UB_RMS,
        MEASURE_UC_RMS,
        MEASURE_UD_RMS,
        MEASURE_IA_RMS,
        MEASURE_IB_RMS,
        MEASURE_IC_RMS,
        MEASURE_INI_RMS,
        MEASURE_INM_RMS,
        MEASURE_INMI_RMS,
        MEASURE_PT,
        MEASURE_PA,
        MEASURE_PB,
        MEASURE_PC,
        MEASURE_QT,
        MEASURE_QA,
        MEASURE_QB,
        MEASURE_QC,
        MEASURE_ST,
        MEASURE_SA,
        MEASURE_SB,
        MEASURE_SC,
        MEASURE_UAF_RMS,
        MEASURE_UBF_RMS,
        MEASURE_UCF_RMS,
        MEASURE_UDF_RMS,
        MEASURE_IAF_RMS,
        MEASURE_IBF_RMS,
        MEASURE_ICF_RMS,
        MEASURE_IMNF_RMS,
        MEASURE_PTF,
        MEASURE_PAF,
        MEASURE_PBF,
        MEASURE_PCF,
        MEASURE_QTF,
        MEASURE_QAF,
        MEASURE_QBF,
        MEASURE_QCF,
        MEASURE_STF,
        MEASURE_SAF,
        MEASURE_SBF,
        MEASURE_SCF,
        MEASURE_FREQ,
        MEASURE_FREQA,
        MEASURE_FREQB,
        MEASURE_FREQC,
        MEASURE_ANGLEA,
        MEASURE_ANGLEB,
        MEASURE_ANGLEC,
        MEASURE_ANGLEN,
        MEASURE_ANGLEVAB,
        MEASURE_ANGLEVAC,
        MEASURE_TYPE_NUM
    } DRV_METROLOGY_MEASURE_TYPE;

## Summary

Identifies all types of measurements.

## Description

Values are calculated both including all harmonics and fundamental only (F added at the end of magnitude name), where:

- U = Voltage RMS value
- I = Current RMS value
- P = Active power value
- Q = Reactive power value
- S = Aparent power value
- FREQ = Frequency of the line voltage fundamental harmonic component determined by the Metrology library using the dominant phase
- ANGLE = Angle between the voltage and current vectors, and between voltage phases

Rev: E