Jump to main content

# 1.1.4.18 DRV_METROLOGY_GetStatusData Function

## C

    DRV_METROLOGY_REGS_STATUS * DRV_METROLOGY_GetStatusData(void);

## Summary

Get the pointer to the status registers of the metrology library application running on the second processor.

## Description

The Metrology library provides information on a set of 32-bit status registers. For a detailed description of the status registers, refer to the `drv_metrology_regs.h` header file.

## Parameters

None.

## Returns

Pointer to the 32-bit metrology status register.

## Example

        /* Get Pointers to metrology data regions */
        app_metrologyData.pMetControl = DRV_METROLOGY_GetControlData();
        app_metrologyData.pMetStatus = DRV_METROLOGY_GetStatusData();
        app_metrologyData.pMetAccData = DRV_METROLOGY_GetAccData();
        app_metrologyData.pMetHarData = DRV_METROLOGY_GetHarData();

## Remarks

None.

Rev: E