Jump to main content

# 2.2.4.5 Multichannel Metrology Driver Configurations

Multichannel Metrology Driver is configured through its MCC component.

Figure 2-48.Mulltichannel Metrology Driver Configuration Overview
A default configuration is provided to handle 3 Voltage channels, 5 Current channels and 3 Powers.
Figure 2-49.Multichannel Driver Default Configuration
Figure 2-50.Channels Configuration
Figure 2-51.Power Source Configuration
Figure 2-52.Advanced Configuration

Rev: E