Jump to main content

# 1.1.4.50 DRV_METROLOGY_AFE_EVENTS Struct

## C

    typedef struct {
        unsigned int paDir : 1;
        unsigned int pbDir : 1;
        unsigned int pcDir : 1;
        unsigned int ptDir : 1;
        unsigned int qaDir : 1;
        unsigned int qbDir : 1;
        unsigned int qcDir : 1;
        unsigned int qtDir : 1;
        unsigned int pafDir : 1;
        unsigned int pbfDir : 1;
        unsigned int pcfDir : 1;
        unsigned int ptfDir : 1;
        unsigned int qafDir : 1;
        unsigned int qbfDir : 1;
        unsigned int qcfDir : 1;
        unsigned int qtfDir : 1;
        unsigned int swellA : 1;
        unsigned int swellB : 1;
        unsigned int swellC : 1;
        unsigned int sagA : 1;
        unsigned int sagB : 1;
        unsigned int sagC : 1;
        unsigned int creepP : 1;
        unsigned int creepPA : 1;
        unsigned int creepPB : 1;
        unsigned int creepPC : 1;
        unsigned int creepQ : 1;
        unsigned int creepQA : 1;
        unsigned int creepQB : 1;
        unsigned int creepQC : 1;
        unsigned int creepIA : 1;
        unsigned int creepIB : 1;
        unsigned int creepIC : 1;
        unsigned int creepS : 1;
        unsigned int phActiveA : 1;
        unsigned int phActiveB : 1;
        unsigned int phActiveC : 1;
        unsigned int reserved : 1;
    } DRV_METROLOGY_AFE_EVENTS;

## Summary

Identifies all events related to metrology library.

## Description

Field description:

- pXDir: Identifies the sign of the active power in channel X. "1" means a negative value, "0" is a positive value.
- qXDir: Identifies the sign of the reactive power in channel X. "1" means a negative value, "0" is a positive value.
- sagX: Voltage Sag Detected Flag for Channel X. "1" means that voltage sag is detected.
- swellX: Voltage Swell Detected Flag for Channel X. "1" means that voltage Swell is detected.
- creepX: Channel X Current or Power Creep Detected Flag. "1" means that Creep is detected.
- phActiveX: Voltage Active Detected Flag for Channel X. "1" means that voltage Active is detected.

Rev: E