Jump to main content

##

# 1.8 USART Driver Asynchronous - USART Echo

This example echoes the received characters over the console using the USART driver in asynchronous mode.

## Description

This example uses the USART driver in asynchronous mode in Bare-Metal and RTOS environment to communicate over the console. It receives and echo’s back the characters entered by the user.

## Downloading and Building the Application

To clone or download this application from Github, go to the main page of this repository and then click Clone button to clone this repository or download as zip file.

Path of the application within the repository is apps/driver/usart/async/usart_echo.

To build the application, refer to the following table and open the project using its IDE.

Project Name | Description
--- | ---
pic32wm_bw1_curiosity.X | MPLAB X project for PIC32WM-BW1 Curiosity board

## Setting Up the Hardware

The following table shows the target hardware for the application projects.

Project Name | Description
--- | ---
pic32wm_bw1_curiosity.X | PIC32WM-BW1 Curiosity board

### Setting Up PIC32WM-BW1 Curiosity Board

- Connect the USB port on the board to the computer using a USB Type-C cable

## Running the Application

1. Open the Terminal application (E.g., Tera term) on the computer.
2. Connect to the USB COM port and configure the serial settings as follows:
   - Baud: 115200
   - Data: 8 Bits
   - Parity: None
   - Stop: 1 Bit
   - Flow Control: None
3. Build and program the application using its IDE.
4. Type a character and observe the output on the console as shown below.
5. LED toggles each time the character is echoed.

Refer to the following table for LED name:

Board | LED Name
--- | ---
PIC32WM-BW1 Curiosity board | Green LED