Jump to main content

##

# DRV_ENCX24J600_ParametersGet Function

## C

    TCPIP_MAC_RES DRV_ENCX24J600_ParametersGet(DRV_HANDLE hMac, TCPIP_MAC_PARAMETERS* pMacParams);

## Returns

- TCPIP_MAC_RES_TYPE_ERR - if the hMac is invalid
- TCPIP_MAC_RES_OK - if the hMac is valid

## Description

ENCX24J600 Get Parameters Get the parameters of the device, which includes that it is an Ethernet device and what it's MAC address is.

## Preconditions

The client had to be successfully opened with DRV_ENCX24J600_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle
pMacParams | pointer to put the parameters