Jump to main content

##

# 1.2.5.1.1 NETCONFIG Configurations

NETCONFIG User Configurations

- Number of Instances:
  - TCPIP Stack Network Interface Count
  - Default value: 1 (Auto-incremented for every new instance is added)
    - The count of network interfaces configured by the user
  - Symbol TCPIP_STACK_NETWORK_INTERAFCE_COUNT

NETCONFIG Instance Specific User Configurations

- Network Configurations Index:

  - TCPIP Stack Network Configuartions Index
  - Default value: (Autofilled)
    - Unique index assigned for every unique instance of NETCONFIG (value starts from 0)
  - Symbol TCPIP_STACK_NETWORK_CONFIG_NUMBER

- Interface:

  - TCPIP Network Default Interface Name
  - Default value: (Autofilled once MAC dependency is satisfied)
  - Symbol TCPIP_NETWORK_DEFAULT_INTERFACE_NAME_IDXn
    - where n respresents Network Configurations Index

- Host Name:

  - TCPIP Network Default Host Name
  - Default value: (Autofilled once MAC dependency is satisfied)
  - Symbol TCPIP_NETWORK_DEFAULT_HOST_NAME_IDXn
    - where n respresents Network Configurations Index

- Mac Address:

  - TCPIP Network Default MAC Address
  - Default value: (Autofilled once MAC dependency is satisfied)
  - Symbol TCPIP_NETWORK_DEFAULT_MAC_ADDR_IDXn
    - where n respresents Network Configurations Index

- IPv4 Static Address:

  - TCPIP Network Default IP Address
  - Default value: 0.0.0.0
  - Symbol TCPIP_NETWORK_DEFAULT_IP_ADDRESS_IDXn
    - where n respresents Network Configurations Index

- IPv4 SubNet Mask:

  - TCPIP Network Default IP Mask
  - Default value: 255.255.255.0
  - Symbol TCPIP_NETWORK_DEFAULT_IP_MASK_IDXn
    - where n respresents Network Configurations Index

- IPv4 Default Gateway Address:

  - TCPIP Network Default Gateway
  - Default value: 0.0.0.0
  - Symbol TCPIP_NETWORK_DEFAULT_GATEWAY_IDXn
    - where n respresents Network Configurations Index

- IPv4 Primary DNS:

  - TCPIP Network Default DNS
  - Default value: 0.0.0.0
  - Symbol TCPIP_NETWORK_DEFAULT_DNS_IDXn
    - where n respresents Network Configurations Index

- Network Configuration Start-up Flags:

  - TCPIP Network Startup Flags
  - Symbol TCPIP_NETWORK_STARTUP_FLAG_IDXn
    - where n respresents Network Configurations Index

- DHCP Flag:

  - TCPIP Network Interface DHCP Flag
  - Default value: "Enable DHCP Client"
  - Symbol TCPIP_NETWORK_INTERFACE_FLAG_DHCP_IDXn
    - where n respresents Network Configurations Index

- DNS Flag:

  - TCPIP Network Interface DNS Flag
  - Default value: "Enable DNS Client"
  - Symbol TCPIP_NETWORK_INTERFACE_FLAG_DNS_IDXn
    - where n respresents Network Configurations Index

- Multicast Enabled on this Interface:

  - TCPIP Network Configure Multicast
  - Default value: False
  - Symbol TCPIP_NETWORK_CONFIG_MULTICAST_IDXn
    - where n respresents Network Configurations Index

- IPv6 Static Address and Subnet Prefix Length:

  - TCPIP Network Interface IPv6 Address Flag
  - Default value: False
  - Symbol TCPIP_NETWORK_INTERFACE_FLAG_IPV6_ADDRESS_IDXn
    - where n respresents Network Configurations Index

- IPv6 Static Address:

  - TCPIP Network Default IPv6 Address
  - Default value: "fde4:8dba:82e1::"
  - Symbol TCPIP_NETWORK_DEFAULT_IPV6_ADDRESS_IDXn
    - where n respresents Network Configurations Index

- IPv6 Static Address Prefix Length:

  - TCPIP Network Default IPv6 Prefix Length
  - Default value: "64"
  - Symbol TCPIP_NETWORK_DEFAULT_IPV6_PREFIX_LENGTH_IDXn
    - where n respresents Network Configurations Index

- IPv6 Default Gateway Address:

  - TCPIP Network Default IPv6 Gateway
  - Default value: ""
  - Symbol TCPIP_NETWORK_DEFAULT_IPV6_GATEWAY_IDXn
    - where n respresents Network Configurations Index

- IPv6 G3-PLC network:

  - TCPIP Network Interafce IPv6 G3-PLC Network Flag
  - Default value: False
  - Symbol TCPIP_NETWORK_INTERFACE_FLAG_IPV6_G3_NET_IDXn
    - where n respresents Network Configurations Index

- G3-PLC router:

  - TCPIP Network Interface IPv6 G3-PLC Network Router Flag
  - Default value: False
  - Symbol TCPIP_NETWORK_INTERFACE_FLAG_IPV6_G3_NET_ROUTER_IDXn
    - where n respresents Network Configurations Index

- G3-PLC router send advertisements:

  - TCPIP Network Interface IPv6 G3-PLC Network Router Advertisements Flag
  - Default value: False
  - Symbol TCPIP_NETWORK_INTERFACE_FLAG_IPV6_G3_NET_ROUTER_ADV_IDXn
    - where n respresents Network Configurations Index

- Advanced Settings:

  - TCPIP Network Advanced Settings
  - Symbol TCPIP_NETWORK_ADV_SETTING_IDXn
    - where n respresents Network Configurations Index

- IPv4 Secondary DNS:

  - TCPIP Network Default Secondary DNS
  - Default value: 0.0.0.0
  - Symbol TCPIP_NETWORK_DEFAULT_SECOND_DNS_IDXn
    - where n respresents Network Configurations Index

- Network MAC Driver:

  - TCPIP Network Default MAC Driver
  - Default value: (Autofilled once MAC dependency is satisfied)
  - Symbol TCPIP_NETWORK_DEFAULT_MAC_DRIVER_IDXn
    - where n respresents Network Configurations Index

- Add Interface to MAC Bridge:

  - TCPIP Network MAC Bridge Add Interface
  - Default value: False
  - Symbol TCPIP_NETWORK_MACBRIDGE_ADD_IDXn
    - where n respresents Network Configurations Index

- Power Mode:

  - TCPIP Network Default Power Mode
  - Default value: "full"
  - Symbol TCPIP_NETWORK_DEFAULT_POWER_MODE_IDXn
    - where n respresents Network Configurations Index