Jump to main content

##

# 1.2.1.16.3 Library Interface

Name | Description
--- | ---
Macros |
TCPIP_REBOOT_MESSAGE | the mesage needed to be sent accross the net to reboot the machine
TCPIP_REBOOT_SAME_SUBNET_ONLY | For improved security, you might want to limit reboot capabilities to only users on the same IP subnet. Define TCPIP_REBOOT_SAME_SUBNET_ONLY to enable this access restriction.
TCPIP_REBOOT_TASK_TICK_RATE | the periodic rate of the Reboot task The default value is 1130 milliseconds. This module listens for incoming reboot requests and a high operation frequency is not required. The value cannot be lower than the TCPIP_STACK_TICK_RATE.
Functions |
TCPIP_REBOOT_Task | Standard TCP/IP stack module task function.
Structures |
TCPIP_REBOOT_CONFIG | TCPIP Reboot server configuration