Jump to main content

##

# DRV_ENC28J60_Status Function

## C

    SYS_STATUS DRV_ENC28J60_Status(SYS_MODULE_OBJ obect);

## Returns

- SYS_STATUS_ERROR - if an invalid handle has been passed in
- SYS_STATUS_UNINITIALIZED - if the driver has not completed initialization
- SYS_STATUS_BUSY - if the driver is closing and moving to the closed state
- SYS_STATUS_READY - if the driver is ready for client commands

## Description

ENC28J60 Status This function will get the status of the driver instance.

## Preconditions

The driver had to be successfully initialized with DRV_ENC28J60_Initialize().

## Parameters

Parameters | Description
--- | ---
object | The object valid passed back to DRV_ENC28J60_Initialize()