Jump to main content

##

# DRV_ETHPHY_CLIENT_STATUS Enumeration

## C

    C
    typedef enum {
        DRV_ETHPHY_CLIENT_STATUS_ERROR,
        DRV_ETHPHY_CLIENT_STATUS_CLOSED,
        DRV_ETHPHY_CLIENT_STATUS_BUSY,
        DRV_ETHPHY_CLIENT_STATUS_READY
    } DRV_ETHPHY_CLIENT_STATUS;

## Description

Ethernet PHY Driver Client Status This enumeration identifies the client-specific status of the Ethernet PHY driver.

- DRV_ETHPHY_CLIENT_STATUS_ERROR - Unspecified error condition
- DRV_ETHPHY_CLIENT_STATUS_CLOSED - Client is not open
- DRV_ETHPHY_CLIENT_STATUS_BUSY - An operation is currently in progress
- DRV_ETHPHY_CLIENT_STATUS_READY - Up and running, no operations running

## Remarks

None.