Jump to main content

##

# DRV_ENCX24J600_Open Function

## C

    DRV_HANDLE DRV_ENCX24J600_Open(SYS_MODULE_INDEX index, DRV_IO_INTENT intent);

## Returns

Returns a valid handle - If successful INVALID_HANDLE - If unsuccessful

## Description

The client will call this function to open a handle to the driver. When the first instance is opened than the driver will send the RX enabled command to the ENC hardware.

## Preconditions

The driver had to be successfully initialized with DRV_ENCX24J600_Initialize.

## Parameters

Parameters | Description
--- | ---
index | This is the index of the driver instance to be initialized. The definition DRV_ENCX24J600_NUM_DRV_INSTANCES controls how many instances are available.
intent | The intent to use when opening the driver. Only exclusive is supported