Jump to main content

##

# DRV_ENCX24J600_PowerMode Function

## C

    bool DRV_ENCX24J600_PowerMode(DRV_HANDLE hMac, TCPIP_MAC_POWER_MODE pwrMode);

## Returns

- false - This functionality is not supported in this version of the driver

## Description

ENCX24J600 Power Mode This function sets the power mode of the ENCX24J600.

## Remarks

This functionality is not implemented in the first release.

## Preconditions

The client had to be successfully opened with DRV_ENCX24J600_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle
pwrMode | the power mode to set