Jump to main content

##

# DRV_ENC28J60_RxFilterHashTableEntrySet Function

## C

    TCPIP_MAC_RES DRV_ENC28J60_RxFilterHashTableEntrySet(DRV_HANDLE hMac, const TCPIP_MAC_ADDR* DestMACAddr);

## Returns

- TCPIP_MAC_RES_TYPE_ERR - if the hMac is invalid
- TCPIP_MAC_RES_OP_ERR - if the hMac is valid

## Description

ENC28J60 Receive Filter Hash Table Entry Set This function adds to the MAC's hash table for hash table matching.

## Remarks

This functionality is not implemented in the first release.

## Preconditions

The client had to be successfully opened with DRV_ENC28J60_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle
DestMACAddr | MAC address to add to the hash table