Jump to main content

##

# TCPIP_IPV6_Get Function

## C

    uint8_t TCPIP_IPV6_Get(
        TCPIP_MAC_PACKET* pRxPkt,
        uint8_t* pData
    );

## Description

This function is used to read the next byte of data from a packet.

## Preconditions

TCPIP_IPV6_Initialize() should be called. TCPIP_IPV6_InterfaceIsReady should be true.

## Parameters

Parameters | Description
--- | ---
pRxPkt | The MAC RX packet to read data from.
pData | Byte data to be read.

## Returns

- 1 - On successful read.
- 0 - No byte is available to read.

## Remarks

None.