Jump to main content

##

# DRV_ETHPHY_HWConfigFlagsGet Function

## C

    DRV_ETHPHY_RESULT DRV_ETHPHY_HWConfigFlagsGet(DRV_HANDLE handle, DRV_ETHPHY_CONFIG_FLAGS* pFlags);

## Returns

DRV_ETHPHY_RES_OK - if the configuration flags successfully stored at pFlags DRV_ETHPHY_RESULT error code otherwise

## Description

This function returns the current Ethernet PHY hardware MII/RMII and ALTERNATE/DEFAULT configuration flags from the Device Configuration Fuse bits.

## Remarks

None.

## Preconditions

- The DRV_ETHPHY_Initialize routine must have been called.

- DRV_ETHPHY_Open must have been called to obtain a valid device handle.

- DRV_ETHPHY_Setup must have been called to properly configure the PHY

## Parameters

Parameters | Description
--- | ---
pFlags | address to store the hardware configuration