Jump to main content

##

# DRV_ENCX24J600_PacketRx Function

## C

    TCPIP_MAC_PACKET* DRV_ENCX24J600_PacketRx(DRV_HANDLE hMac, TCPIP_MAC_RES* pRes, const TCPIP_MAC_PACKET_RX_STAT** ppPktStat);

## Returns

- Pointer to a valid packet - if successful
- NULL - if unsuccessful

## Description

ENCX24J600 Receive Packet This function retrieves a packet from the driver. The packet needs to be acknowledged with the linked acknowledge function so it can be reused.

## Remarks

ppPktStat is ignored in the first release.

## Preconditions

The client had to be successfully opened with DRV_ENCX24J600_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle
pRes | the result of the operation
ppPktStat | pointer to the receive statistics