Jump to main content

##

# DRV_ETHPHY_ClientOperationAbort Function

## C

    DRV_ETHPHY_RESULT DRV_ETHPHY_ClientOperationAbort(DRV_HANDLE handle);

## Returns

- DRV_ETHPHY_RESULT value describing the current operation result: DRV_ETHPHY_RES_OK for success; operation has been aborted an DRV_ETHPHY_RESULT error code if the operation failed.

## Description

Aborts a current client operation initiated by the Ethernet PHY driver.

## Remarks

None

## Preconditions

- The DRV_ETHPHY_Initialize routine must have been called.
- DRV_ETHPHY_Open must have been called to obtain a valid opened device handle.
- A driver operation was started