Jump to main content

##

# TCPIP_DHCPV6_IA_STATE Enumeration

## C

    typedef enum {
    TCPIP_DHCPV6_IA_STATE_SOLICIT,
    TCPIP_DHCPV6_IA_STATE_REQUEST,
    TCPIP_DHCPV6_IA_STATE_DAD,
    TCPIP_DHCPV6_IA_STATE_DECLINE,
    TCPIP_DHCPV6_IA_STATE_BOUND,
    TCPIP_DHCPV6_IA_STATE_RENEW,
    TCPIP_DHCPV6_IA_STATE_REBIND,
    TCPIP_DHCPV6_IA_STATE_CONFIRM,
    TCPIP_DHCPV6_IA_STATE_RELEASE,
    TCPIP_DHCPV6_IA_STATE_ERROR_TRANSIENT,
    TCPIP_DHCPV6_IA_STATE_ERROR_FATAL,
    TCPIP_DHCPV6_IA_STATE_NUMBER
    } TCPIP_DHCPV6_IA_STATE;

## Description

IA run states.

## Members

Members | Description
--- | ---
TCPIP_DHCPV6_IA_STATE_SOLICIT | Solicitation.
TCPIP_DHCPV6_IA_STATE_REQUEST | Perform request.
TCPIP_DHCPV6_IA_STATE_DAD | Start the DAD state.
TCPIP_DHCPV6_IA_STATE_DECLINE | Decline the DAD addresses.
TCPIP_DHCPV6_IA_STATE_BOUND | Bound.
TCPIP_DHCPV6_IA_STATE_RENEW | Renew address.
TCPIP_DHCPV6_IA_STATE_REBIND | Rebind address.
TCPIP_DHCPV6_IA_STATE_CONFIRM | Confirm address.
TCPIP_DHCPV6_IA_STATE_RELEASE | Release address.
TCPIP_DHCPV6_IA_STATE_ERROR_TRANSIENT | An error ocurred for which either user intervention is required.
TCPIP_DHCPV6_IA_STATE_ERROR_FATAL | Fatal error occurred; not properly configured options/buffers, etc.
TCPIP_DHCPV6_IA_STATE_NUMBER | Number of run states.