Jump to main content

##

# DRV_ETHMAC_Tasks_ISR Function

## C

    void DRV_ETHMAC_Tasks_ISR(SYS_MODULE_OBJ macIndex);

## Returns

None.

## Description

This is the Ethernet MAC driver interrupt service routine. It processes the Ethernet related interrupts and notifies the events to the driver user (the TCP/IP stack).

## Remarks

None.

## Preconditions

DRV_ETHMAC_PIC32MACInitialize() should have been called. The TCP/IP stack event notification should be enabled.