Jump to main content

##

# 2.1.8 Interrupt Configuration

The NVIC (Nested Vectored Interrupt Controller) is the interrupt controller in SAM devices. For other devices, refer the interrupt section in device datasheet.

1. Start NVIC Configuration from Plugins drop-down menu
2. Verify whether GMAC(Ethernet MAC) interrupt is enabled.
3. Apart from the interrupt shown in the image, GMAC_Q1 to GMAC_Q5 will be enabled for SAME70/SAMV71 devices.