Jump to main content

##

# 1.2.4.7.3 Library Interface

Name | Description
--- | ---
Macros |
TCPIP_IPV6_MTU_INCREASE_TIMEOUT | 600 seconds
TCPIP_IPV6_NDP_DELAY_FIRST_PROBE_TIME | 5 s
TCPIP_IPV6_NDP_MAX_ANYCAST_DELAY_TIME | 1 s
TCPIP_IPV6_NDP_MAX_MULTICAST_SOLICIT | 3 transmissions
TCPIP_IPV6_NDP_MAX_NEIGHBOR_ADVERTISEMENT | 3 transmissions
TCPIP_IPV6_NDP_MAX_RTR_SOLICITATION_DELAY | 1 s
TCPIP_IPV6_NDP_MAX_RTR_SOLICITATIONS | 3 transmissions
TCPIP_IPV6_NDP_MAX_UNICAST_SOLICIT | 3 transmissions
TCPIP_IPV6_NDP_REACHABLE_TIME | 30 s
TCPIP_IPV6_NDP_RETRANS_TIMER | 1 s
TCPIP_IPV6_NDP_RTR_SOLICITATION_INTERVAL | 4 s
TCPIP_IPV6_NDP_TASK_TIMER_RATE | The NDP task rate, milliseconds The default value is 32 milliseconds. The lower the rate (higher the frequency) the higher the module priority and higher module performance can be obtained The value cannot be lower than the TCPIP_STACK_TICK_RATE.
TCPIP_IPV6_NDP_VALID_LIFETIME_TWO_HOURS | Sets the lifetime to 2 hours
Reachability Functions |
TCPIP_NDP_NborReachConfirm | Confirms that a neighbor is reachable