Jump to main content

##

# TCPIP_DHCPV6_IA_SUBSTATE Enumeration

## C

    typedef enum {
    TCPIP_DHCPV6_IA_SUBSTATE_START,
    TCPIP_DHCPV6_IA_SUBSTATE_IDELAY,
    TCPIP_DHCPV6_IA_SUBSTATE_TRANSMIT,
    TCPIP_DHCPV6_IA_SUBSTATE_WAIT_REPLY,
    TCPIP_DHCPV6_IA_SUBSTATE_NUMBER
    } TCPIP_DHCPV6_IA_SUBSTATE;

## Description

IA run substates most IA run states that must send a message go through these substates.

## Members

Members | Description
--- | ---
TCPIP_DHCPV6_IA_SUBSTATE_START | Message start/preparation.
TCPIP_DHCPV6_IA_SUBSTATE_IDELAY | Message wait for iDelay.
TCPIP_DHCPV6_IA_SUBSTATE_TRANSMIT | Send/transmit message.
TCPIP_DHCPV6_IA_SUBSTATE_WAIT_REPLY | Wait message reply.
TCPIP_DHCPV6_IA_SUBSTATE_NUMBER | Number of standard message sub-states.