Jump to main content

##

# DRV_MIIM_OPERATION_CALLBACK Type

## C

    typedef void (* DRV_MIIM_OPERATION_CALLBACK)(DRV_HANDLE cliHandle, DRV_MIIM_OPERATION_HANDLE opHandle, DRV_MIIM_RESULT opResult, uint16_t opData);

## Description

Type: MIIM Driver Operation Complete Callback The format of an operation callback notification function registered with the MIIM driver.

## Remarks

None.

## Parameters

Parameters | Description
--- | ---
cliHandle | the client handle. This is the handle that identifies the client (obtained with DRV_MIIM_Open) that initiated the operation.
opHandle | the operation handle. This is the handle that identifies the operation (obtained with DRV_MIIM_Read, DRV_MIIM_Write, etc.)
opResult | operation result DRV_MIIM_RES_OK if operation completed successfully, otherwise an error code
opData | operation specific data, only if the result is DRV_MIIM_RES_OK For read/scan operation this is the MIIM read data. For write operation this is that data that was written with MIIM.