Jump to main content

##

# DRV_ENCX24J600_Status Function

## C

    SYS_STATUS DRV_ENCX24J600_Status(SYS_MODULE_OBJ obect);

## Returns

- SYS_STATUS_ERROR - if an invalid handle has been passed in
- SYS_STATUS_UNINITIALIZED - if the driver has not completed initialization
- SYS_STATUS_BUSY - if the driver is closing and moving to the closed state
- SYS_STATUS_READY - if the driver is ready for client commands

## Description

ENCX24J600 Status This function will get the status of the driver instance. The driver had to be successfully initialized with DRV_ENCX24J600_Initialize().

## Parameters

Parameters | Description
--- | ---
object | The object valid passed back to DRV_ENCX24J600_Initialize()