Jump to main content

##

# TCPIP_DHCP_IsActive Function

## C

    bool TCPIP_DHCP_IsActive(
        TCPIP_NET_HANDLE hNet
    );

## Description

This function returns the current state of the DHCP client on the specified interface.

## Preconditions

DHCP module should have been initialized.

## Parameters

Parameters | Description
--- | ---
hNet | Interface to query.

## Returns

- True - If the DHCP client service is currently active on the specified interface.
- False - If the DHCP client service is not active on the specified interface.

## Remarks

The DHCP client service could be enabled bot not active. For example when there was no DHCP server detected on the network.