Jump to main content

##

# TCPIP_TFTPC_EVENT_TYPE Enumeration

## C

    typedef enum {
        TFTPC_EVENT_NONE = 0,
        TFTPC_EVENT_PUT_REQUEST = 0x0001,
        TFTPC_EVENT_GET_REQUEST = 0x0002,
        TFTPC_EVENT_ACKED = 0x0004,
        TFTP_EVENT_DATA_RECEIVED = 0x0008,
        TFTPC_EVENT_DECLINE = 0x0010,
        TFTPC_EVENT_TIMEOUT = 0x0020,
        TFTPC_EVENT_COMPLETED = 0x0040,
        TFTPC_EVENT_CONN_LOST = 0x0080,
        TFTPC_EVENT_CONN_ESTABLISHED = 0x0100,
        TFTPC_EVENT_SERVICE_DISABLED = 0x0200,
        TFTPC_EVENT_BUSY = 0x0400
    } TCPIP_TFTPC_EVENT_TYPE;

## Description

Enumeration: TCPIP_TFTPC_EVENT_TYPE.

None.

## Members

Members | Description
--- | ---
TFTPC_EVENT_NONE = 0 | TFTP no event.
TFTPC_EVENT_PUT_REQUEST = 0x0001 | TFTP PUT request sent.
TFTPC_EVENT_GET_REQUEST = 0x0002 | TFTP GET request sent.
TFTPC_EVENT_ACKED = 0x0004 | TFTP request acknowledge was received.
TFTP_EVENT_DATA_RECEIVED = 0x0008 | TFTP client received data for GET request.
TFTPC_EVENT_DECLINE = 0x0010 | TFTP file PUT or GET communication declined due to bad PDU.
TFTPC_EVENT_TIMEOUT = 0x0020 | TFTP server timeout.
TFTPC_EVENT_COMPLETED = 0x0040 | TFTP file PUT or GET completed.
TFTPC_EVENT_CONN_LOST = 0x0080 | Connection the the TFTP server lost.
TFTPC_EVENT_CONN_ESTABLISHED = 0x0100 | Connection re-established.
TFTPC_EVENT_SERVICE_DISABLED = 0x0200 | TFTP service disabled.
TFTPC_EVENT_BUSY = 0x0400 | TFTP client communication is going on.