Jump to main content

##

# TCPIP_ARP_RESULT Enumeration

## C

    typedef enum {
    ARP_RES_OK = 0,
    ARP_RES_ENTRY_NEW,
    ARP_RES_ENTRY_SOLVED,
    ARP_RES_ENTRY_QUEUED,
    ARP_RES_ENTRY_EXIST,
    ARP_RES_PERM_QUOTA_EXCEED,
    ARP_RES_PROBE_OK,
    ARP_RES_NO_ENTRY = -1,
    ARP_RES_CACHE_FULL = -2,
    ARP_RES_TX_FAILED = -3,
    ARP_RES_BAD_INDEX = -4,
    ARP_RES_BAD_ADDRESS = -5,
    ARP_RES_NO_INTERFACE = -6,
    ARP_RES_BAD_TYPE = -7,
    ARP_RES_CONFIGURE_ERR = -8,
    ARP_RES_PROBE_FAILED = -9
    } TCPIP_ARP_RESULT;

## Description

Enumeration: TCPIP_ARP_RESULT.

Various definitions for success and failure codes.

## Members

Members | Description
--- | ---
ARP_RES_OK = 0 | Operation succeeded.
ARP_RES_ENTRY_NEW | Operation succeeded and a new entry was added.
ARP_RES_ENTRY_SOLVED | The required entry is already solved.
ARP_RES_ENTRY_QUEUED | The required entry was already queued.
ARP_RES_ENTRY_EXIST | The required entry was already cached.
ARP_RES_PERM_QUOTA_EXCEED | Info: the quota of permanent entries was exceeded.
ARP_RES_PROBE_OK | Requested probe sent.
ARP_RES_NO_ENTRY = -1 | No such entry exists.
ARP_RES_CACHE_FULL = -2 | The cache is full and no entry could be removed to make room.
ARP_RES_TX_FAILED = -3 | Failed to transmit an ARP message.
ARP_RES_BAD_INDEX = -4 | Bad query index.
ARP_RES_BAD_ADDRESS = -5 | Bad IP address specified.
ARP_RES_NO_INTERFACE = -6 | No such interface exists.
ARP_RES_BAD_TYPE = -7 | No such type is valid/exists.
ARP_RES_CONFIGURE_ERR = -8 | Interface is configuring now, no ARP probes.
ARP_RES_PROBE_FAILED = -9 | Requested probed failed.

## Remarks

None.