Jump to main content

##

# TCPIP_DNSS_RESOLVE_TYPE Enumeration

## C

    typedef enum {
    TCPIP_DNSS_TYPE_A = 1,
    TCPIP_DNSS_TYPE_MX = 15,
    TCPIP_DNSS_TYPE_AAAA = 28u,
    TCPIP_DNSS_TYPE_ANY = 0xff
    } TCPIP_DNSS_RESOLVE_TYPE;

## Description

Enumeration: TCPIP_DNSS_RESOLVE_TYPE

This enumeration lists the RecordType argument for TCPIP_DNSS_Resolve. The stack supports DNSS_TYPE_A and DNSS_TYPE_AAAA.

## Members

Members | Description
--- | ---
TCPIP_DNSS_TYPE_A = 1 | Indicates an A (standard address) record.
TCPIP_DNSS_TYPE_MX = 15 | Indicates an MX (mail exchanger) record.
TCPIP_DNSS_TYPE_AAAA = 28u | Indicates a quad-A (IPv6 address) address record.

## Remarks

None.