Jump to main content

##

# MAC_DRVR_Tasks_ISR Function

## C

    void MAC_DRVR_Tasks_ISR( SYS_MODULE_OBJ macIndex );

## Returns

None

## Description

This is the Ethernet MAC driver interrupt service routine. It processes the Ethernet related interrupts and notifies the events to the driver user, the TCP/IP stack.

## Remarks

None

## Preconditions

- MAC_DRVR_Initialize() should have been called.
- The TCP/IP stack event notification should be enabled.

## Parameters

Parameters | Description
--- | ---
macIndex | Parameter identifying the intended MAC client