Jump to main content

##

# TCPIP_DHCPS_REQ_FORMAT_ERR_MASK Enumeration

## C

    typedef enum
    {
    TCPIP_DHCPS_REQ_FORMAT_ERR_NONE = 0,
    TCPIP_DHCPS_REQ_FORMAT_ERR_SRV_ID_SET = 0x0001,
    TCPIP_DHCPS_REQ_FORMAT_ERR_SRV_ID_MISS = 0x0002,
    TCPIP_DHCPS_REQ_FORMAT_ERR_REQUEST_IP_SET = 0x0004,
    TCPIP_DHCPS_REQ_FORMAT_ERR_REQUEST_IP_MISS = 0x0008,
    TCPIP_DHCPS_REQ_FORMAT_ERR_CIADDR_ERR = 0x0010,
    }TCPIP_DHCPS_REQ_FORMAT_ERR_MASK;

## Description

DHCPs error mask for a TCPIP_DHCPS_EVENT_REQ_FORMAT_ERROR event

List of errors that can be signaled by a TCPIP_DHCPS_EVENT_REQ_FORMAT_ERROR event. More that one error could be set.

## Members

Members | Description
--- | ---
TCPIP_DHCPS_REQ_FORMAT_ERR_NONE | no error occurred
TCPIP_DHCPS_REQ_FORMAT_ERR_SRV_ID_SET | server identifier set when it should have been cleared
TCPIP_DHCPS_REQ_FORMAT_ERR_SRV_ID_MISS | server identifier missing when it should have been set
TCPIP_DHCPS_REQ_FORMAT_ERR_REQUEST_IP_SET | requested IP address set when it should have been cleared
TCPIP_DHCPS_REQ_FORMAT_ERR_REQUEST_IP_MISS | requested IP address missing
TCPIP_DHCPS_REQ_FORMAT_ERR_CIADDR_ERR | wrong 'ciaddr' field