Jump to main content

##

# PPP_GetState Function

## C

    bool PPP_GetState(DRV_HANDLE hMac, PPP_STATE state[2]);

## Returns

true - if the call succeeded

false - if there was an error

## Description

This function gets the PPP current state for the LCP and IPCP

## Remarks

None

## Preconditions

The PPP module must be initialized.

## Parameters

hMac - driver handle (obtained by calling TCPIP_MAC_Open/DRV_PPP_MAC_Open)

state - address to receive the current LCP and IPCP states. Must be able to hold both instances.