Jump to main content

##

# DRV_ENCX24J600_ConfigGet Function

## C

    size_t DRV_ENCX24J600_ConfigGet(DRV_HANDLE hMac, void* configBuff, size_t buffSize, size_t* pConfigSize);

## Returns

Number of bytes copied to the buffer ENCX24J600 Get Configuration Gets the current configuration.

## Remarks

This function does nothing in the first release.

## Preconditions

The client had to be successfully opened with DRV_ENCX24J600_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle
configBuff | location to copy the configuration too
buffSize | buffer size
pConfigSize | configuration size needed