Jump to main content

##

# 1.2.1.1.2 TCPIP Announce Configurations

Announce Specific User Configurations

- Announce Broadcast Type:

  - Type of the broadcast used by the Announce module
  - This type enables the network directed broadcast
  - If it is not defined or it is 0, the network limited broadcast is used
  - The default is nework limited broadcast
  - Default value: 0
  - Symbol TCPIP_ANNOUNCE_NETWORK_DIRECTED_BCAST

- Announce Task Rate (in msec):

  - Announce task processing rate, in milliseconds.
  - The Announce module will process a timer event with this rate for maintaining its own queues, processing timeouts, etc.
  - The lower the rate (higher the frequency) the higher the module priority and higher module performance can be obtained
  - The value cannot be lower than the TCPIP_STACK_TICK_RATE.
  - Default value: 333
  - Symbol TCPIP_ANNOUNCE_TASK_RATE

- Maximum Payload Size:

  - Maximum size of a payload sent once
  - Adjust to your needs
  - Default value: 512
  - Symbol TCPIP_ANNOUNCE_MAX_PAYLOAD