Jump to main content

##

# 1.2.1.16.2 TCPIP Reboot Configurations

Reboot Specific User Configurations

- Allow Only Same Subnet:

  - For improved security, you might want to limit reboot capabilities to only users on the same IP subnet.
  - Defining this symbol enables this access restriction.
  - Default value: true
  - Symbol TCPIP_REBOOT_SAME_SUBNET_ONLY

- Reboot Message:

  - The mesage needed to be sent accross the net to reboot the machine
  - Default value: "MCHP Reboot"
  - Symbol TCPIP_REBOOT_MESSAGE

- Reboot Task Rate (in msec):

  - Reboot task processing rate, in milliseconds.
  - The lower the rate (higher the frequency) the higher the module priority and higher module performance can be obtained
  - The value cannot be lower than the TCPIP_STACK_TICK_RATE.
  - The Reboot module just listens for incoming reboot requests
  - A high operation frequency is not required.
  - Default value: 1130
  - Symbol TCPIP_REBOOT_TASK_TICK_RATE