Jump to main content

##

# 1 Harmony 3 Peripheral Library Application Examples for PIC32MZ DA Family

The following applications are provided to demonstrate the typical or interesting usage models of one or more peripheral libraries.

Name | Description
--- | ---
ADCHS DMA | This example application shows how to sample an analog input using the ADCHS peripheral and displays the converted samples on a serial terminal.
ADCHS Interrupt | This example application shows how to sample an analog input using the ADCHS peripheral and displays the converted samples on a serial terminal
ADCHS Polling | This example application shows how to sample an analog input using the ADCHS peripheral and displays the converted samples on a serial terminal
Cache Maintenance Operations | This example demonstrates the cache maintenance operation by cleaning and invalidating the cache for the DMA buffers located in the cacheable SRAM region
CMP Configurable Reference | This example application shows how to use the CMP Peripheral library to compare voltage level on the negative input with the internal configurable reference voltage
CORETIMER Periodic Interrupt | This example application shows how to use the CoreTimer to generate periodic interrupts
DMAC Memory Transfer | This example application demonstrates how to use the DMAC peripheral to do a memory to memory transfer
DMAC USART Echo | This example application demonstrates USART transfer with DMA to receive 10 bytes and echo back the received bytes
DMT Timeout | This example application shows how the deadman timer resets by not clearing the deadman timer counter on switch press
GPIO Interrupt | This example application demonstrate how to generate GPIO interrupt on switch press and release, and indicate the switch status using the LED
GPIO Polling | This example application demonstrate how to poll the switch input, and indicate the switch status using the LED
I2C EEPROM Read Write | This example application demonstrates how to use the I2C peripheral to write and read from the I2C serial EEPROM memory
ICAP Capture Mode | This example application shows how to use the ICAP peripheral to measure the pulse width of the input signal
NVM Flash Read Write | This example application demonstrates how to use the NVM to erase and program the internal Flash memory
OCMP Compare Mode | This example application shows how to use the OCMP peripheral to generate an active low, active high, and toggle output on compare match
RNG Random Number | This example application shows how to use the RNG Peripheral library to generate a pseudo-random number
RTCC Alarm Interrupt | This example application shows how to use the RTCC to configure the time and generate the alarm
SPI Blocking | This example application demonstrates how to use the SPI peripheral to transmit and receive a block of data in a blocking manner
SPI Interrupt | This example application demonstrates how to use the SPI peripheral to transmit and receive a block of data using interrupt
SQI Flash Read Write | This example application demonstrates how to use the SQI Peripheral library to perform erase, write and read operation with the SQI Serial Flash memory
TMR Periodic Interrupt | This example demonstrates how to use the TMR module in timer mode to generate periodic interrupt
TMR1 Periodic Interrupt | This example demonstrates how to use the TMR1 module in timer mode to generate periodic interrupt
UART Echo Blocking | This example application demonstrates how to use the UART peripheral to transfer a block of data in a blocking manner
UART Echo Interrupt | This example application demonstrates how to use the UART peripheral to transfer a block of data in a non-blocking manner
UART Ring Buffer | This example application demonstrates how to use the UART peripheral in ring buffer mode
WDT Timeout | This example application shows how the watchdog timer resets by not feeding the watchdog on switch press