Jump to main content

##

# 1 Harmony 3 Peripheral Library Application Examples for SAM L10/L11 Family

The following applications are provided to demonstrate the typical or interesting usage models of one or more peripheral libraries.

Name | Description
--- | ---
AC Sleepwalking | This example application shows how to use the AC Peripheral library to perform a single shot comparison in standby sleep mode periodically and wake up the device at the end of a successful comparison
ADC DMA Sleepwalking | This application shows how to configure the ADC in a sleepwalking operation, where the input voltage is measured at a fixed interval, and then the device is woken from sleep after conversion of 16 samples
ADC Window Sleepwalking | This application shows how to configure ADC in a sleepwalking operation, where input voltage is measured at a fixed interval, but device is not woken from sleep until the measured value is below a given threshold
Clock Configuration | This example application shows how to configure the clock system to run the device at maximum frequency. It also outputs a prescaled clock signal on a GPIO pin for measurement and verification
DAC Waveform Generation | This example application shows how to use the DAC to generate a 1 kHz Sine or Sawtooth wave with a look up table
DAC Waveform Generation with DMA | This example application shows how to use the DAC with the DMA to generate a 5 kHz sinusoidal waveform without CPU intervention
DMAC Memory Transfer | This example application demonstrates how to use the DMAC peripheral to do a memory to memory transfer
DMAC USART Echo | This example application demonstrates USART transfer with DMA to receive 10 bytes and echo back the received bytes
DSU Compute CRC32 | This example application demonstrates how to use the DSU Peripheral library to compute 32-bit Cyclic Redundancy Checksum (CRC)
EIC Interrupt | This example application demonstrates how to generate interrupt using the EIC on switch press and indicate it through an LED
EVSYS Trigger | This example application demonstrates how to use the EVSYS Peripheral library to setup autonomous, low-latency and configurable communication between peripherals
FREQM Measurement | This example application demonstrates how to use the FREQM peripheral to measure the frequency of the internal RC Oscillator
NVMCTRL Read Write | This example application demonstrates how to use the NVMCTRL to erase and program the internal Flash memory
OPAMP ADC Gain | This application shows how OPAMP can be used as gain stage for the internal ADC peripheral
PM Wakeup Using EIC | This application demonstrates entering the low power modes and exiting it using the EIC
PM Wakeup Using RTC | This example demonstrates entering the low power modes and exiting it using the RTC
PORT Polling | This example application demonstrate how to poll the switch input, and indicate the switch status using the LED
RSTC Reset Cause | This example shows how to use the RSTC peripheral to indicate the cause of the device reset
RTC Alarm Interrupt | This example shows how to use the RTC to configure the time and generate the alarm
RTC Periodic Interrupt | This example application shows how to use the RTC to generate periodic interrupts
RTC Tamper Detect | This example application shows how to configure and use tamper detect feature of RTC
SERCOM I2C EEPROM Emulation (I2C Client) | This example application demonstrates how to use the SERCOM peripheral in client mode
SERCOM I2C EEPROM Read Write | This example application demonstrates how to use the SERCOM peripheral to write and read from the I2C serial EEPROM memory
SERCOM SPI Blocking | This example application demonstrates how to use the SERCOM SPI peripheral to transmit and receive a block of data in a blocking manner
SERCOM SPI EEPROM Read Write | This example application demonstrates how to use the SERCOM SPI peripheral to write and read from the SPI serial EEPROM memory
SERCOM SPI Interrupt | This example application shows how to use SERCOM SPI PLIB with external loop back to write and then read back an array of data in interrupt mode
SERCOM SPI Ping Pong with DMA | This example demonstrates how to continuously transmit and receive data over a SPI interface using ping pong buffers with DMA
SERCOM USART Blocking | This example application demonstrates how to use the SERCOM peripheral in USART mode to transfer block of data in a blocking manner
SERCOM USART Interrupt | This example application demonstrates how to use the SERCOM peripheral in USART mode to transfer data in a non-blocking manner
SERCOM USART Ring Buffer | This example application demonstrates how to use the SERCOM peripheral in USART ring buffer mode to transfer data in a non-blocking manner
Systick Periodic Interrupt | This example shows how to use the SysTick to generate periodic interrupts
TC Capture Mode | This example shows how to use the TC module in capture mode to measure duty cycle and frequency of an external input
TC Compare Mode | This example shows how to use the TC module in compare mode to generate an active low, active high, and toggle output on compare match
TC Timer Mode | This example shows how to use the TC module in timer mode to generate periodic interrupt
TRAM Erase On Tamper Detect | This example application shows how to configure and use tamper detect feature of RTC and TrustRam
TRNG Random Number | This example shows how to use the TRNG Peripheral library to generate and read a random number
TrustZone Basic Demonstration | This example application performs Add and Multiply Math operations in secure mode and I/O operations in non-secure mode
TrustZone EIC Pin Toggle | This example application demonstrates handling of external pin interrupt in secure and non-secure project
TrustZone EVSYS Trigger | This example application demonstrates peripheral event handling with event system in secure and non-secure project
TrustZone Systick Periodic Timeout | This example application shows how to use the SysTick to generate periodic interrupts on both Secure and Non-secure modes
WDT Timeout | This example shows how to generate a Watchdog timer reset by emulating a deadlock