Jump to main content

# 4.3 New Device Support

(Ask a Question)

## 4.3.1 RT PolarFire FPGA

(Ask a Question)

### 4.3.1.1 New RTPF500ZT/TS/TL/TLS Devices

(Ask a Question)

Libero SoC v2024.1 introduces the following devices.

Table 4-1.RTPF500ZT/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage | Timing/Power
--- | --- | --- | --- | ---
RTPF500ZT/TS/TL/TLS | MIL | STD / -1 | 1.0V, 1.05V | Preliminary

PF_SYSTEM_SERVICES core adds support to handle the sNVM page size differences in RTPF500ZT/TS/TL/TLS devices when compared to MPF500T/TS/TL/TLS devices.

Power Up to Functional (PUFT) timing numbers have been updated in the Design Initialization report for RTPF500ZT/TS/TL/TLS devices to account for ECC usage on data stored in internal sNVM.

For information about RTPF500ZT/LS/TL/TLS devices, see AN4903: Differences Between RT PolarFire RTPF500T and RTPF500ZT FPGAs.

## 4.3.2 PolarFire SoC

(Ask a Question)

### 4.3.2.1 New TGrade2 Packages

(Ask a Question)

Libero SoC v2024.1 introduces the following production packages:

Table 4-2.New TGrade2 Packages
Device | Packages | Temp-range | Speed-grade
--- | --- | --- | ---
MPFS095T | FCSG536 | TGrade2 | STD, -1
MPFS160T | FCSG536 | TGrade2 | STD, -1
MPFS250T | FCSG536 | TGrade2 | STD, -1
MPFS250T | FCG1152 | TGrade2 | STD, -1

Attention: TGrade2 temp-range for the MPFS460T device has been withdrawn.

### 4.3.2.2 FCG1152 Packages for MPFS460T/TS/TL/TLS

(Ask a Question)

Libero SoC v2024.1 introduces the FCG1152 production package, which replaces the corresponding FCG1152_EVAL package for the following devices.

Table 4-3.FCG1152 Packages for MPFS460T/TS/TL/TLS
Device | Package | Speed-grade
--- | --- | ---
MPFS460T/TS | FCG1152 | STD, -1
MPFS460TL/TLS | FCG1152 | STD

Attention: The conversion is automatic if you open an existing design containing the EVAL package. However, Tcl scripts must be changed to use the new package name.

Rev: 2025.2

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.