Jump to main content

# 7.3 New Device Support

(Ask a Question)

## 7.3.1 PolarFire

(Ask a Question)

### 7.3.1.1 Automotive T2 Grade for MPF500TS

(Ask a Question)

Libero SoC v2023.1 introduces Automotive T2 Grade for MPF500TS.

Table 7-1.Automotive T2 Grade for MPF500TS
Device | Temp-range | Speed-grade | Voltage | Timing and Power
--- | --- | --- | --- | ---
MPF500TS | T2 Grade | STD, -1 | 1.0V, 1.05V | Production

Rev: 2026.1

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.