Jump to main content

# 1.4.1 PolarFire, PolarFire SoC, RT PolarFire, and RT PolarFire SoC

(Ask a Question)

## 1.4.1.1 Simulation Model Enhancements

(Ask a Question)

The Libero SoC v2025.2 release has the following updates and enhancements to PolarFire Simulation models:

- Added post-layout back-annotated simulation support for Differential input I/O.
- Added simulation support for wide-mode programmable input delay taps in PF_IO and PF_IOD_GENERIC_RX cores.

## 1.4.1.2 IOD Octal DDR Enhancements

(Ask a Question)

Libero SoC v2025.2 introduces several enhancements to improve configurability, timing, and simulation accuracy for IOD Octal DDR:

- PLL_POWERDOWN_N is now exposed by default to facilitate enabling of the PLL only when the REF_CLK input is stable.
- Added DQS_DELAY_TAP options up to 139 for expanded tuning flexibility.
- Any tap value in the full range of 1–255 allowed for the DQS delay setting.
- Added support for non-integer clock frequency entry to accommodate a wider range of design requirements.
- Improved timing constraints generation to ensure better coverage and timing robustness.
- Improved performance by inserting two-stage pipeline and register duplication for Async-assert, Sync-deassert Reset.

## 1.4.1.3 IOD RX Updates

(Ask a Question)

The Libero SoC v2025.2 release enables Expose fractional clock parallel data in the Fractional Dynamic mode.

## 1.4.1.4 Added Failsafe ODT_EN Support for SPACEWIRE_RX

(Ask a Question)

Libero SoC v2025.2 adds the option to expose the Failsafe ODT_EN port for the SPACEWIRE_RX core interface.

## 1.4.1.5 Added DLL Register in the Design Initialization Report

(Ask a Question)

The Libero SoC v2025.2 release adds DLL register details in the Design Initialization report.

## 1.4.1.6 Added Support for Initial Static Delay on Dynamically Tuned I/O Interfaces

(Ask a Question)

Libero SoC v2025.2 allows IN_DELAY and OUT_DELAY options in PDC and I/O Editor for Dynamic I/O interfaces (except DDR, LPDDR, QDR, CDR) to set the initial startup delay value, which can be dynamically tuned during operation.

## 1.4.1.7 Enhanced PF_SRAM_AHBL_AXI with High-Reliability Options

(Ask a Question)

Libero SoC v2025.2 adds new options for high reliability to enable fault tolerance logic, synchronous reset, and timeout counts for read and write operations on the AHBL or AXI interface.

## 1.4.1.8 Enabled Fault Tolerance for PF_SYSTEM_SERVICES

(Ask a Question)

The Libero SoC v2025.2 release adds new options for high reliability to enable fault tolerance logic in the PF_SYSTEM_SERVICES core.

## 1.4.1.9 CoreAXI4Interconnect and CoreAHB-Lite Cores

(Ask a Question)

Libero SoC v2025.2 refreshes the Memory Map definitions with the new initiator and target terminologies for CoreAXI4Interconnect and CoreAHB-Lite cores.

## 1.4.1.10 Expanded Live Probe Trigger Controls in SmartDebug

(Ask a Question)

Libero SoC v2025.2 adds support for selecting trigger signal’s edge in SmartDebug when a signal is assigned to Live Probe that acts as a trigger.

## 1.4.1.11 Upgraded Silver License to Add Support for MPF200T-FCG784

(Ask a Question)

The Libero SoC 2025.2 release upgrades the Silver license for MPF200T device (FCG784 package), with extended device range enabled.

Rev: 2025.2

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.