Jump to main content

# 8.3 New Device Support

(Ask a Question)

## 8.3.1 PolarFire

(Ask a Question)

### 8.3.1.1 Production Timing and Power for MPF050T/TS/TL/TLS

(Ask a Question)

Table 8-1 8-2 8-4.PolarFire Production Timing and Power for MPF050T/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPF050T/TS | EXT, IND | -1 | 1.0V, 1.05V
MPF050T/TS/TL/TLS | EXT, IND | STD | 1.0V, 1.05V

### 8.3.1.2 Automotive T2 Grade for MPF050T

(Ask a Question)

Table 8-1 8-2 8-4.PolarFire Automotive T2 Grade Production Timing and Power
Device | Temp-range | Voltage | Timing and Power
--- | --- | --- | ---
MPF050T | STD, -1 | 1.0V, 1.05V | Preliminary

### 8.3.1.3 Programming and SmartDebug for MPF050T/TS/TL/TLS

(Ask a Question)
Libero SoC v2022.2 introduces programming and SmartDebug support for the following PolarFire devices:

- MPF050T/TS/TL/TLS

### 8.3.1.4 FCVG484 and FCSG325 Packages for MPF050T/TS/TL/TLS

(Ask a Question)
Libero SoC v2022.2 introduces the FCVG484, FCSG325 production packages, which replace the corresponding FCVG484_EVAL, FCSG325_EVAL packages for the MPF050T/TS/TL/TLS devices.
Note: The conversion is automatic if you open an existing design containing the EVAL package. However, user Tcl scripts must be changed to use the new package names.

Table 8-3.FCVG484 and FCSG325 Packages for MPF050T/TS/TL/TLS
Device | Package | Speed-grade
--- | --- | ---
MPF050T/TS | FCVG484, FCSG325 | STD, -1
MPF050TL/TLS | FCVG484, FCSG325 | STD

## 8.3.2 PolarFire SoC

(Ask a Question)

### 8.3.2.1 Preliminary Timing and Power for MPFS095T/TS/TL/TLS

(Ask a Question)

Table 8-1 8-2 8-4.PolarFire SoC Preliminary Timing and Power for MPFS095T/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPFS095T/TS | EXT, IND | -1 | 1.0V, 1.05V
MPFS095T/TS/TL/TLS | EXT, IND | STD | 1.0V, 1.05V
MPFS095T | T2 Grade | STD, -1 | 1.0V, 1.05V
MPFS095TS MIL | MIL | STD | 1.0V, 1.05V

### 8.3.2.2 Preliminary Timing and Power for MPFS160T/TS/TL/TLS

(Ask a Question)

Table 8-5.Preliminary Timing and Power for MPFS160T/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPFS160T/TS | EXT, IND | -1 | 1.0V, 1.05V
MPFS160T/TS/TL/TLS | EXT, IND | STD | 1.0V, 1.05V
MPFS160T | T2 Grade | STD, -1 | 1.0V, 1.05V

### 8.3.2.3 Preliminary Timing and Power for MPFS460T/TS/TL/TLS

(Ask a Question)

Table 8-6.Preliminary Timing and Power for MPFS460T/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPFS460T/TS | EXT, IND | -1 | 1.0V, 1.05V
MPFS460T/TS/TL/TLS | EXT, IND | STD | 1.0V, 1.05V
MPFS460T | T2 Grade | STD, -1 | 1.0V, 1.05V
MPFS460TS | MIL | STD | 1.0V, 1.05V

### 8.3.2.4 Programming for MPFS160T/TS/TL/TLS

(Ask a Question)
Libero SoC v2022.2 introduces programming support for the following PolarFire SoC devices:

- MPFS160T/TS/TL/TLS

### 8.3.2.5 FCVG484 Packages for MPFS095T/TS/TL/TLS and MPFS0160T/TS/TL/TLS

(Ask a Question)
Libero SoC v2022.2 introduces the FCVG484 production packages, which replace the corresponding FCVG484_EVAL package for the following devices.
Important: The conversion is automatic if you open an existing design containing the EVAL package. However, user Tcl scripts must be changed to use the new package names.

Table 8-7.FCVG484 Packages for MPFS095T/TS/TL/TLS and MPFS0160T/TS/TL/TLS
Device | Package | Speed-grade
--- | --- | ---
MPFS095T/TS | FCVG484 | STD, -1
MPFS095TL/TLS | FCVG484 | STD
MPFS160T/TS | FCVG484 | STD, -1
MPFS160TL/TLS | FCVG484 | STD

## 8.3.3 SmartFusion2

(Ask a Question)

### 8.3.3.1 New 158 FCSG Package for M2S025

(Ask a Question)

Table 8-8.New 158 FCSG Package for M2S025
Device | Package | Speed | Platinum | Gold | Evaluation | Silver
--- | --- | --- | --- | --- | --- | ---
M2S025 | FCSG158 | -1, STD | yes | yes | yes | no

Rev: 2025.2

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.